Dora Juan Juan HU

[jjhu@i2r.a-star.edu.sg](mailto:jjhu@i2r.a-star.edu.sg)

Institute for Infocomm Research, Agency for Science, Technology and Research (A\*STAR), Singapore

Ying Cui

[YCUI2@e.ntu.edu.sg](mailto:YCUI2@e.ntu.edu.sg)

School of Electrical and Electronic Engineering, Nanyang Technological University, Singapore

XLIM research institute UMR CNRS University of Limoges, France CINTRA CNRS/NTU/THALES, UMI 3288, Research Techno Plaza, 50 Nanyang Drive, Border X Block, Level 6, Singapore 637553

Jun Long Lim

[jllim@i2r.a-star.edu.sg](mailto:jllim@i2r.a-star.edu.sg)

Institute for Infocomm Research, Agency for Science, Technology and Research (A\*STAR), Singapore

Perry Ping Shum

[epshum@ntu.edu.sg](mailto:epshum@ntu.edu.sg)

School of Electrical and Electronic Engineering, Nanyang Technological University, Singapore

Georges Humbert

georges.humbert@xlim.fr

XLIM research institute UMR CNRS University of Limoges, France

Jean-Louis Auguste

[jean-louis.auguste@xlim.fr](mailto:jean-louis.auguste@xlim.fr)

XLIM research institute UMR CNRS University of Limoges, France

Yixin Wang

[wangyx@i2r.a-star.edu.sg](mailto:wangyx@i2r.a-star.edu.sg)

Institute for Infocomm Research, Agency for Science, Technology and Research (A\*STAR), Singapore